( TL19E00F18100000000FAAT02 )

EPS Symptom Troubleshooting - EPS indicator does not go off, and no DTCs are stored

1. Measure the voltage between EPS control unit connector D (28P) terminal No. 16 and body ground.

Is there battery voltage?

YES | - | Go to Step 8 .
NO | - | Repair open in the wire between the EPS control unit and driver's under-dash fuse/relay box.■

1. Turn the ignition switch to LOCK (0).

1. Disconnect the EPS control unit connector A (2P).