( TL19E00J26220230115KBAT00 )

Glove Box Lock Cylinder Replacement

NOTE: Take care not to scratch the glove box.

1. Remove the glove box.

1. Lift the glove box handle (A), and use a release one end of the retainer (B) from its slot.
   NOTE:
   - Do not remove the retainer entirely. Leave one end of the retainer in its original position when removing the lock cylinder.
   - LHD model: Use a hook-shaped tool to pull the middle of the retainer.
   - RHD model: Use a flat-tip screwdriver to push out the end of the retainer.

LHD model
RHD model