( TL19E1AE34116317081KBAT00 )

Clutch Slave Cylinder Replacement

NOTE:

- Use fender covers to avoid damaging painted surfaces.
- Do not spill brake fluid on the vehicle; it may damage the paint or plastic. If brake fluid does contact the paint or plastic, wash it off immediately with water.
- The illustration show K24Z3 engine model.

1. Disconnect the clutch line (A) from the slave cylinder (B). To prevent spills, cover the line joint with rags or shop towels.
   NOTE: Loosen the flare nut (C) while holding the clutch line connector (D) with a wrench.

1. Remove the slave cylinder from the transmission housing.