( TL19E1AE34151150941MFAT00 )

M/T Reverse Lockout Solenoid Disassembly/Reassembly

1. Remove the intake air duct: R20A3 engine model, K24Z3 engine model.

1. Remove the air cleaner housing: R20A3 engine model, K24Z3 engine model.

1. Carefully remove the shift cables, and cable bracket together to avoid bending the shift cables: R20A3 engine model, K24Z3 engine model.

1. Disconnect the reverse lockout solenoid 2P connector (A).

1. Remove the reverse lockout solenoid (B).