( TL19E1AE34116300000KBAT00 )

Clutch Replacement

Special Tools Required
Slide hammer weight
07741-0010201
Bearing remover shaft
07936-3710600
Driver handle, 15 x 135L
07749-0010000
Bearing driver attachment, 22 x 24 mm
07746-0010800
Ring gear holder
07LAB-PV00100
Shaft (clutch alignment tool),
07PAF-0020100
Taper cone (clutch alignment tool),
07PAF-0020200
Clutch alignment pilot, 21 mm
07PAF-0020370
Remover handle
07936-3710100
NOTE: The illustrations show K24Z3 engine model.
Engine Side
Pressure Plate Inspection and Removal

1. Remove the transmission: R20A3 engine model, R24Z3 engine model.

1. Check the height evenness of the diaphragm spring fingers using the dial indicator (A). If the most measurement difference is more than the service limit, replace the pressure plate.

   Standard (New): | 0.6 mm (0.02 in.) max.
   Service Limit: | 0.8 mm (0.03 in.)