( TL19E00J26200016101KBAT00 )

Carpet Replacement

SRS components are located in this area. Review the SRS component locations and the precautions and procedures before doing repairs or service.
NOTE:

- Put on gloves to protect your hands.
- Take care not to damage, wrinkle or twist the carpet.
- Be careful not to damage the dashboard and other interior trim pieces.
- When removing components, use the trim tools or equivalent.

1. Remove the front seat mounting bolts.

1. Do the battery terminal disconnection procedure, then wait at least 3 minutes before beginning work.

1. Remove these items:
   - Front seats, both sides
   - Rear seat cushion
   - Front door sill trim, both sides
   - Rear door sill trim, both sides
   - Front door opening seal, as needed
   - Rear door opening seal, as needed
   - Kick panels, both sides
   - Center pillar lower trim
   - Driver's dashboard undercover
   - Passenger's dashboard undercover, for some models
   - Center console panel
   - Center console rear trim
   - Driver's center trim
   - Passenger's dashboard trim
   - Passenger's center trim
   - Center console
   - Rear ventilation ducts, both sides, for some models
   - Steering joint cover
   - Parking brake lever
   - Driver's dashboard center lower cover
   - Passenger's dashboard center lower cover
   - M/T model: Shift lever bracket
   - A/T model: Shift lever

1. Remove the front passenger's seat belt lower anchor bolt.

1. Release the hooks (A), then remove the accelerator pedal clip (B).