( TL19E1AE34150100000LDAT00 )

M/T Assembly Reassembly

1. Install three 14 x 20 mm dowel pins (A).

1. Place the transmission housing on the clutch housing, being careful to line up the shafts.

1. While expanding the 72 mm snap ring (B) on the countershaft ball bearing using the snap ring pliers, push the transmission housing down to start the countershaft ball bearing through the snap ring.
   Then release the pliers, and push down the housing until it bottoms and the snap ring snaps in place in the countershaft ball bearing snap ring groove.
   NOTE: Install the 32 mm sealing cap (C) after setting in the 72 mm snap ring.