( TL19E00J18526228101KBAT00 )

Fuel Pipe Protector Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the body.

1. Remove the left rear wheel.

1. Remove the clips, then remove the fuel pipe protector (A).

1. Install the protector in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips into place securely.