( TL19E00J2621651640CKDAT00 )

Center Console Inner Box Lid Removal/Installation

NOTE:

- Take care not to scratch the center console and the related parts.
- When removing components, use the trim tools or equivalent.

1. Remove the center console panel.

1. Disconnect the rear accessory power socket connector, and if equipped, the auxiliary jack assembly connector and the USB jack connector.

1. Open the console armrest.

1. Remove the console box mat (A).
   NOTE: It is easier to use packing tape to remove the mat.

1. Remove the screws, then open the lid (A) by prying the hooks (B) with the appropriate trim tool.

1. Pivot the Inner box lid (A) up on the upper hooks (B) to detach the lower hook (C), then remove the lid from the console box (D).

1. Install the lid in the reverse order of removal.