( TL19E00J54400020371KBAT10 )

Front Door Glass and Regulator Replacement

NOTE: Put on gloves to protect your hands.

1. Remove these items:
   - Tweeter cover
   - Door panel

1. Raise the glass fully.

1. Remove the screws, then remove the door panel bracket (A).

1. Disconnect the power door lock actuator connector (A) and the power mirror connectors (B), and detach the power mirror connector and the harness clip (C). Remove the plug caps (D).

1. Pass the wire harnesses (E) through the slits (F) in the plastic cover (G), then remove the plastic cover.
   NOTE: Remove the glue from the door surface. If the plastic cover is damaged or torn, replace it.

1. Carefully raise the glass (A) until you can see the bolts, then remove them. Carefully pull the glass out through the window slot. Take care not to drop the glass inside the door.

1. Disconnect the connector (A) from the regulator (B).

1. Remove the bolts and the nuts, then remove the regulator through the hole in the door.

1. Apply multipurpose grease to all the sliding surfaces of the regulator (A) where shown.

1. Install the glass and regulator in the reverse order of removal, and note these items:
   - Roll the glass up and down to see if it moves freely without binding.
   - Make sure that there is no clearance between the glass and glass run channel when the glass is closed.
   - Adjust the position of the glass as necessary.
   - Do the power window control unit reset procedure.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.
   - Check for water leaks.
   - Test-drive and check for wind noise and rattles.
   - Make sure the power door locks, windows and power mirror operate properly.