( TL19E00J16126721513KBAT00 )

Front Door Sash Outer Trim Replacement

NOTE: Take care not to scratch the door.

1. Remove these items:
   - Tweeter cover
   - Door panel
   - Power mirror
   - Door outer molding

1. Pull the door sash outer trim (A) up to release the hooks (B) from the door, and release the trim from between the door glass outer weatherstrip (C) and the door, then remove the trim. Take care not to damage the door glass outer weatherstrip.

1. Install the trim in the reverse order of removal.