( TL19E1PE10410654801FEAT00 )

A/T Shift Solenoid Valve Test

1. Disconnect the shift solenoid wire harness connector.

1. Measure the resistance:
   - No. 1 terminal: Shift solenoid valve C
   - No. 2 terminal: Shift solenoid valve B
   - No. 3 terminal: Shift solenoid valve E
   - No. 5 terminal: Shift solenoid valve A
   - No. 8 terminal: Shift solenoid valve D

   Standard: | 12−25 Ω

   - If the resistance is within the standard, go to Step 9 .
   - If the resistance is out of standard, go to Step 10 .

1. Connect a jumper wire from the negative battery terminal to body ground, and connect another jumper wire from the positive battery terminal to each shift solenoid wire harness connector terminal individually. A clicking sound should be heard.
   - If a clicking sound is heard, the valves are OK. The test is complete, reconnect the connector, and install all removed parts.
   - If no clicking sound is heard, go to Step 10 .