( TL19E00B20200014202MDAT00 )

Ball Joint Boot Inspection/Replacement

1. The front upper arm ball joint: Adjust the ball joint boot clip guide with the adjusting bolt (A) until its base is just above the groove around (B) the bottom of the boot. Then slide the clip (C) over the ball joint boot clip guide and into position on the boot.

1. After installing a boot, wipe any grease off the exposed portion of the ball joint pin.

1. Install all the removed parts.