( TL19E20A18300043401KCAT00 )

Engine Oil Pan Installation

1. Tighten the bolts in three steps. In the final step, tighten all bolts, in sequence, to 18 N·m (1.8 kgf·m, 13 lbf·ft). Wipe off the excess liquid gasket on the each side of crankshaft pulley and the flywheel/drive plate.
   NOTE:
   - Wait at least 30 minutes before filling the engine with oil.
   - Do not run the engine for at least 3 hours after installing the oil pan.