( TL19E10K791000R121XFAAT00 )

DTC Troubleshooting: 12-1x

1. Check for continuity between the No. 2 and the No. 3 terminals of the dashboard wire harness 4P connector.

Is there continuity?

YES | - | Faulty SRS unit or poor connection at SRS unit connector A (39P) and the SRS unit. Check the connection between the connector and the SRS unit. If the connection is OK, replace the SRS unit. ■
NO | - | Open in the dashboard wire harness; replace the dashboard wire harness.■