( TL19E00K764000Y1125FAAT00 )

DTC Troubleshooting: B1125

DTC B1125:
Driver's Power Window Motor Pulse A Error

1. Clear the DTCs with the HDS.

1. Turn the ignition switch to LOCK (0) and then back to ON (II).

1. Open and close the driver's power window by using the power window master switch manually.

Does the window motor operate?

YES | - | Go to Step 4 .
NO | - | Test the driver's power window motor. ■

1. Check for DTCs with the HDS.

Is DTC B1125 indicated?

YES | - | Go to Step 5
NO | - | Intermittent failure, the system is OK at this time. Check for loose or poor connections.■

1. Select the POWER WINDOWS from the BODY ELECTRICAL system select menu, and enter the DATA LIST.

1. Check the DETECT/NONE information of the driver's window motor A-phase pulse signal in the DATA LIST.

Does the information indicator display DETECT while the window is moving, and display NONE when the window is stopped?

YES | - | Replace the power window master switch.■
NO | - | Go to Step 7 .

1. Check for DTCs with the HDS.

Is DTC B1126 also indicated?

YES | - | Go to Step 14 .
NO | - | Go to Step 8 .

1. Turn the ignition switch to LOCK (0).

1. Disconnect the door multiplex control unit 37P connector.

1. Disconnect the driver's power window motor 6P connector.

1. Check for continuity between the door multiplex control unit 37P connector No. 22 terminal and driver's power window motor 6P connector No. 6 terminal.

Is there continuity?

YES | - | Go to Step 12 .
NO | - | Repair an open in the wire.■