( TL19E00J46127053676KBAT00 )

Front Seat Frame Replacement

Driver's Seat
NOTE:

- Put on gloves to protect your hands.
- When removing components, use the trim tools or equivalent.
- If the side airbag has deployed, replace the seat frame and related parts with new ones.
- LHD model is shown; RHD model is symmetrical.

1. Remove the front seat.

1. Remove these items:
   - Front seat-back cover/pad
   - Front seat cushion cover/pad
   - Seat belt buckle
   - Side airbag

1. Except manual seat: Detach the clips (A, B), then remove the upper rail outer cover (C).

8-way power seat
Manual height adjustable seat