( TL19E00K75200081070FAAT00 )

DTC Troubleshooting: 7

LKAS Camera DTC 7:
High Temperature Detection with LKAS Camera

1. Start the engine.

1. Set the temperature control button to Max Cool, the mode control button to Vent and the recirculation control button to Recirculate.

1. Turn the A/C button on and fan button to Max, and running the air conditioning for 15 minutes or more.

1. Clear the DTCs with the HDS.

1. Stop the engine.

1. Check for DTCs with the HDS.

Is DTC 7 indicated?

YES | - | Check for loose terminals in the LKAS camera 10P connector. If all connections are OK, replace the LKAS camera. ■
NO | - | Intermittent failure, the system is OK at this time.■