( TL19E00H46400026001KBAT00 )

E-pretensioner Unit Replacement

NOTE: Do not turn the ignition switch to ON (II) while the E-pretensioner unit connectors are disconnected.

1. Remove the driver's dashboard lower cover.

1. Disconnect the connectors (A) from the E-pretensioner unit (B).

1. Remove the mounting bolts (C), then pull out the E-pretensioner.

1. Install the unit in the reverse order of removal.

1. After installing, make sure the SRS indicator comes on for about 6 seconds after turning the ignition switch ON (II), then goes off.