( TL19E00J26220219245KDAT00 )

Dashboard Side Defogger Vent Trim Removal/Installation

NOTE:

- Take care not to scratch the dashboard and its related parts.
- When removing components, use the trim tools or equivalent.
- The left side defogger vent trim is shown; the right side defogger vent trim is symmetrical.

1. Insert the appropriate trim tool into a gap between the side defogger vent trim (A) and the dashboard, and pry the hook (B).

1. Pull out the trim to release the tab (C), then remove the trim.

1. Install the tab portion of the trim first, then push the hook into place securely.