( TL19E00K75100081190FAAT00 )

DTC Troubleshooting: 19

1. Check for continuity between LKAS control unit 26P connector No. 7 terminal and LKAS camera 10P connector No. 6 terminal.

Is there continuity?

YES | - | Check for loose terminals in the LKAS camera and LKAS control unit connectors, then repair if necessary. If all connections are OK, replace the LKAS camera. ■
NO | - | Repair an open in the wire between LKAS camera and LKAS control unit.■