( TL19E00K75100081080FAAT00 )

DTC Troubleshooting: 8, 14

1. Check for continuity between LKAS control unit 26P connector No. 25 terminal and ECM/PCM connector A (49P) No. 4 terminal.

Is there continuity?

YES | - | Check for loose terminals in the ECM/PCM connector and LKAS control unit connector, and repair if necessary. If all connections are OK, replace the ECM/PCM. ■
NO | - | Repair an open in the wire between the LKAS control unit and the branch of the F-CAN line (CANL).■