( TL19E1PE10400013015KBAT00 )

ATF Filter Replacement

1. Disconnect the ATF cooler/filter hoses (A) from the ATF filter (B), then plug the hoses.

1. Remove the ATF filter holder (C) and the ATF filter.

1. Install a new ATF filter on the ATF filter mounting bracket (D), and secure it with its holder and bolt. Remove the plugs from the hose.

1. Slide the ATF cooler hose on the ATF filter until they touch the filter housing, and secure the hose with the clips (E) at 6−8 mm (0.24−0.31 in.) (F) from the filter housing.