( TL19E00K791000R421XFAAT00 )

DTC Troubleshooting: 42-1x

1. Measure the resistance between the No. 38 terminal of SRS unit connector A (39P) and body ground, and between the No. 39 terminal and body ground. There should be an open circuit or at least 1 MΩ.

Is the resistance as specified?

YES | - | Go to Step 12 .
NO | - | Short to ground in the right engine compartment wire harness or dashboard wire harness; replace the faulty harness.■

1. Do the battery terminal reconnection procedure.

1. Turn the ignition switch to ON (II).