( TL19E30A14680200000KAAT00 )

Cylinder Head Valve, Spring, and Valve Seal Removal

Special Tools Required
Valve spring compressor attachment
07757-PJ10100
Valve spring compressor
07757-0010000
Identify the valves and the valve springs as they are removed so that each item can be reinstalled in its original position.

1. Remove the cylinder head.

1. Using an appropriate-sized socket (A) and a plastic mallet (B), lightly tap the spring retainer to loosen the valve cotters.

1. Install the valve spring compressor and the attachment. Compress the spring, and remove the valve cotters.

1. Remove the valve spring compressor and the attachment, then remove the spring retainer, the valve spring, the valve seal, and the valve spring seat.