( TL19E00J16166221401KDAT00 )

Rear Door Panel Removal/Installation

1. Remove the door panel (A) with as little bending as possible to avoid creasing or breaking it.

   -1. | Start at the bottom edge of the door panel, release the clips that are just above the marks (B) on the edge of the panel with a commercially available trim pad remover.
   -2. | Detach the upper clips.
   -3. | Starting at the rear, pull the door panel upward. NOTE: The inner handle cable (C) and the latch cable (D) are connected to the inner handle (E). Do not pull the door panel up too far, or these cables will be damaged.