( TL19E1PE10410612223FEAT10 )

A/T Clutch Pressure Control Solenoid Valve A Test

1. Remove the harness clamps (B) from the clamp brackets.

1. Remove the bolts (C) securing the ATF cooler inlet line (D).

1. Remove the mounting bolts and A/T clutch pressure control solenoid valve A.

1. Remove the ATF pipe (E), the ATF joint pipes (F), the O-rings (G), and the gasket (H).

1. Check the fluid passage of A/T clutch pressure control solenoid valve A for contamination.
   If necessary, clean the A/T clutch pressure control solenoid valve body.