( TL19E00B54100000000BAAT00 )

The Extraction of the Fluid Sealant of the Tyre Inflator

1. Bend and bind up the tube of the bottle (A) that is filled with the fluid sealant as shown in the figure.

1. If you reuse the tyre, completely wipe up the fluid sealant sat around the drain hole, fix a flat, and replace the valve.
   NOTE:
   - Wipe the fluid sealant completely so that the beaded edge of the tyre and the mating portion of the wheel rim and the bead are cleared.
   - The damaged portion such as punctures may be filled with the fluid sealant, and can not be found depending on the extent of the damage.
   - If you drive on a flat tyre, often check the tyre pressure and replace the tyre with a normal one when you detect any abnormality (air pressure reduction in the tyre).