( TL19E00J16126720801KBAT00 )

Front Door Latch Replacement

1. Disconnect the latch cable (A) and the inner handle cable (B) from the latch (C).

1. Install the latch in the reverse order of removal, and note these items:
   - Make sure the actuator connector is plugged in properly and each rod is connected securely.
   - Make sure the door locks and opens properly.
   - When reinstalling the door panel, make sure the plastic cover is installed properly and sealed around its outside perimeter to seal out water.