( TL19E00J10300027201FHAT00 )

Speaker Test/Replacement

Front Center Speaker (With Premium Audio System)

1. Remove the speaker lid (A).

1. Remove the bolts, then pull out the front center speaker (B).

1. Disconnect the 2P connector (C), and remove the front center speaker.

1. Measure the resistance between the No. 1 and No. 2 terminals. There should be about 4 Ω.

1. If the resistance is not as specified, replace the front center speaker.