( TL19E00E16236500000LCAT00 )

Intermediate Shaft Disassembly

Special Tools Required
Half shaft base
07NAF-SR30101
Oil seal driver, 44.5 mm
07947-SB00100
NOTE: The illustrations show K24Z3 engine model.

1. K24Z3 engine model: Remove the heat shield (A).

1. Remove the outer seal (A) and the external snap ring (B) from the intermediate shaft (C).

1. Press the intermediate shaft (A) out of the intermediate shaft bearing (B) using the half shaft base (C) and a press. Be careful not to damage the bearing support ring (D) on the intermediate shaft during disassembly.

1. Remove the internal snap ring (A) from the bearing support (B).

1. Press the intermediate shaft bearing (A) out of the bearing support (B) using the 44.5 mm oil seal driver (C), the half shaft base (D), and a press.