( TL19E1AE34150700000MBAT00 )

M/T Differential Thrust Clearance Adjustment

1. Measure clearance between 80 mm shim and the bearing outer race in the transmission housing.

   Standard: | 0−0.10 mm (0−0.0039 in.)

1. If the clearance is more than the standard, select a new 80 mm shim from the following table. If the clearance measured in Step 6 is within the standard, go to Step 10 .
   80 mm Shim

   Type | Part Number | Thickness
   --- | --- | ---
   A | 41441-PL3-B00 | 1.00 mm (0.039 in.)
   B | 41442-PL3-B00 | 1.10 mm (0.043 in.)
   C | 41443-PL3-B00 | 1.20 mm (0.047 in.)
   D | 41444-PL3-B00 | 1.30 mm (0.051 in.)
   E | 41445-PL3-B00 | 1.40 mm (0.055 in.)
   F | 41446-PL3-B00 | 1.50 mm (0.059 in.)
   G | 41447-PL3-B00 | 1.60 mm (0.063 in.)
   H | 41448-PL3-B00 | 1.70 mm (0.067 in.)
   J | 41449-PL3-B00 | 1.80 mm (0.071 in.)
   K | 41450-PL3-B00 | 1.05 mm (0.041 in.)
   L | 41451-PL3-B00 | 1.15 mm (0.045 in.)
   M | 41452-PL3-B00 | 1.25 mm (0.049 in.)
   N | 41453-PL3-B00 | 1.35 mm (0.053 in.)
   P | 41454-PL3-B00 | 1.45 mm (0.057 in.)
   Q | 41455-PL3-B00 | 1.55 mm (0.061 in.)
   R | 41456-PL3-B00 | 1.65 mm (0.065 in.)
   S | 41457-PL3-B00 | 1.75 mm (0.069 in.)

1. Remove the bolts and transmission housing.

1. Replace the thrust shim selected in Step 7 , then recheck the clearance.

1. Install the new left driveshaft side oil seal to the transmission housing.

1. Reinstall the transmission housing.