( TL19E00F00000057111KDAT00 )

Steering Gearbox Removal and Installation

1. K24Z3 engine A/T model: Remove the upper base bracket (A) from the base bracket (B).

1. Raise the vehicle on a lift.

1. Remove the front splash shield.

1. Remove the exhaust pipe A:
   - R20A3 engine model
   - K24Z3 engine model

1. A/T: Disconnect the shift cable from the selector control lever.

1. With the HID lamp model: Disconnect the suspension stroke sensor connector.