( TL19E1PE10410424251KCAT00 )

A/T End Cover Installation

1. Install a new gasket (B) on the transmission housing, and install the ATF pipe (C) and the ATF joint pipes (D).
   NOTE: Be sure to install a new gasket with the blue side toward the transmission housing.

1. Install a new O-rings (E) over the ATF joint pipes, and install A/T clutch pressure control solenoid valve A.

1. Check the fluid passage of A/T clutch pressure control solenoid valves B and C for contamination. If necessary, clean the A/T clutch pressure control solenoid valve body.

1. Clean the mounting surface and fluid passage of the transmission housing.