( TL19E00H32500000000FAAT12 )

LKAS Symptom Troubleshooting - LKAS indicator (orange) does not come on

LKAS indicator (orange) does not come on

1. Turn the ignition switch to ON (II).

1. Watch the following indicators in the gauge control module:
   - Malfunction indicator lamp (MIL)
   - Brake system indicator
   - Charging indicator

Do the indicators come on?

YES | - | Go to the gauge control module self-diagnostic function. ■
NO | - | Go to Step 3 .

1. Turn the ignition switch to LOCK (0).

1. Check the No. 5 (7.5 A) fuse in the driver's under-dash fuse/relay box.

Is the fuse OK?

YES | - | Go to Step 5 .
NO | - | Replace the fuse, then recheck.■

1. Disconnect gauge control module 32P connector.

1. Turn the ignition switch to ON (II).

1. Check for voltage between the gauge control module 32P connector No. 15 terminal and body ground.

Is there battery voltage?

YES | - | Substitute a known-good gauge control module and recheck. If the problem goes away, replace the original gauge control module. ■
NO | - | Repair an open in the wire, if the wire is OK, replace the driver's under-dash fuse/relay box. ■