( TL19E00R311000K5352YDAT02 )

Front Wheelhouse/Damper Housing Removal

NOTE: This section explains the procedures after removal of all accessories and related parts. For accessories' and related parts' removal procedure, refer to the appropriate Shop Manual.
Mass production body welding position and number (Wheelhouse upper member and wheelhouse upper inner)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Mass production body welding position and number (Front wheelhouse and damper housing)
NOTE:

- Welding symbols
  : 2-Plate spot welding/ : 3-Plate spot welding/ : 4-Plate spot welding/ : MIG plug welding/ : MIG welding L= Welding length Unit: mm (in.)
- ( ): The number of welds

Construction

- Remove the wheelhouse upper member.
- Replace the wheelhouse upper inner and the lower member as an assembly, and check the wheelhouse lower member support position for damage. If necessary, replace it.
- Check the damper position for damage. If necessary, replace the front wheelhouse and the damper housing.