( TL19E00H46400055412KBAT00 )

Side Impact Sensor (First) Replacement

Removal

1. Do the battery terminal disconnection procedure, then wait for 3 minutes before starting work.

1. Remove the front seat assembly.

1. Remove the center pillar lower trim panel.

1. Disconnect the SRS floor wire harness 2P connector (A) from the side impact sensor (first).

1. Using a TORX T30 bit, remove the TORX bolt (B), then remove the side impact sensor (first) (C).