( TL19E3AE34150700000MAAT00 )

M/T Differential Backlash Inspection

K24Z3 Engine Model

1. Install the driveshaft and intermediate shaft into the differential assembly.

1. Carefully clamp the driveshaft (A) in a vise (B).

1. Place the intermediate shaft (C) on a V-block (D), then fix the intermediate shaft using a vise or equivalent (E).

1. Measure the backlash of the final driven gear (F) with a dial indicator (G). When the backlash is not within the standard, check the differential carrier condition, and replace it if necessary.

   Standard (New): | 0.8−1.3 mm (0.031−0.051 in.)