( TL19E00K791000R411XFAAT00 )

DTC Troubleshooting: 41-1x

1. Measure the voltage between the No. 36 terminal of SRS unit connector A (39P) and body ground, and between the No. 37 terminal and body ground. There should be less than 1 V.

Is the voltage as specified?

YES | - | Go to Step 15 .
NO | - | Short to power in the left engine compartment wire harness or dashboard wire harness; replace the faulty harness.■

1. Turn the ignition switch to LOCK (0).