( TL19E00J26273455795KDAT00 )

Interior Trim Removal/Installation - Trunk Area

With Temporary Repair Kit (TRK)/With Compact Spare Tyre
NOTE:

- Put on gloves to protect your hands.
- Take care not to bend or scratch the trim and the panels.
- When removing components, use the trim tools or equivalent.

1. Fold both the rear seat-backs forward.

1. For some models: Pull back the front portion of the spare tyre lid (A), and detach the clips.