( TL19E00J46161854027KBAT00 )

Front Seat Recline Motor Replacement

1. Remove the bolt, then remove the recline motor (A). The driver's seat on LHD model is shown; the passenger's seat is symmetrical; the ones on RHD model are similar.

1. Install the motor in the reverse order of removal, and note these items:
   - Replace the push nut with a new one. Make sure the push nut is installed correctly.
   - Make sure the recline motor harness is routed properly.
   - Apply medium strength liquid thread lock to the mounting bolt before reinstallation.