( TL19E00J18513415011KDAT00 )

Front Bumper Removal/Installation

1. If equipped, disconnect the front fog light connectors (A), the headlight washer tube (B), and the front corner sensor connector (C) while holding the front bumper (D), then remove the bumper.

1. Install the bumper in the reverse order of removal, and note these items:
   - If equipped, make sure the front fog light connectors and the front corner sensor connector are plugged in properly, and the headlight washer tube is connected properly.
   - Make sure the front bumper engages the hooks (of both upper beams and side spacers) on each side securely.
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Push the clips and the hooks into place securely.