( TL19E1PE10411619605MAAT00 )

A/T Differential Carrier Bearing Preload Inspection

1. Install the 76 mm thrust shim (A) in the transmission housing (B). If you replace the 76 mm thrust shim with a new one, use the same thickness shim as the old one.

1. Install the 76.2 mm thrust washer (C) and the bearing outer race (D) in the transmission housing.
   NOTE: Be sure to install the 76.2 mm thrust washer with the ‘‘41382 RKY'' mark facing downward.