( TL19E00J16166222051KBAT00 )

Rear Door Weatherstrip Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the door.
- Take care not to damage the front upper corner clip (black) and the rear upper corner clips (black) in the weatherstrip because these clips are not able to replace with new ones.
- Use a clip remover to remove the clips.

1. At the center pillar, remove the door checker mounting bolt (A).

1. Detach the clips (B, C, D), and release the door weatherstrip (E) from the holder (F) of the door sash, then remove the weatherstrip.

1. Install the weatherstrip in the reverse order of removal, and note these items:
   - If the clips are damaged or stress-whitened, replace them with new ones.
   - Make sure the weatherstrip is installed in the holder securely.
   - Apply medium strength liquid thread lock to the door checker mounting bolt before installation.
   - Check for water leaks.