( TL19E00F00000057101MAAT00 )

Steering Column Inspection

Inspection

1. Remove the steering column.

1. Do these checks:
   - Check for loose bearing mounting nuts (A). If they are loosed, replace the column as an assembly.
   - Check the steering column ball bearings (B) and the steering joints (C) for play and proper movement. If any bearing is noisy or has excessive play, replace the steering column as an assembly.
   - Check the sliding capsules (D) for distortion or breakage. If there is distortion or breakage, replace the steering column as an assembly.
   - Check the tilt mechanism and telescopic mechanism for movement and damage.

1. Install the steering column.

Inspection

1. Remove the steering column.

1. Do these checks:
   - Check for loose bearing mounting nuts (A). If they are loosed, replace the column as an assembly.
   - Check the steering column ball bearings (B) and the steering joints (C) for play and proper movement. If any bearing is noisy or has excessive play, replace the steering column as an assembly.
   - Check the sliding capsules (D) for distortion or breakage. If there is distortion or breakage, replace the steering column as an assembly.
   - Check the tilt mechanism and telescopic mechanism for movement and damage.

1. Install the steering column.

Check of Tilting Force

1. Set the steering wheel in the straight driving position, and loosen the lock lever fully.

1. Attach the spring scale to the highest point of the steering wheel, and tilt the steering column to the lowest position.

1. Pull the spring scale straight up, and read the force required to move the steering column.

1. Attach the spring scale to the lowest point of the steering wheel.

1. Pull the spring scale straight down, and read the force required to move the steering column.

   Tilting force (upward/downward):
   Standard: | 70 N (7.1 kgf, 15 lbf) max.

1. If the measurement is higher than the specified, replace the steering column as an assembly.

Check of Telescoping Force

1. Set the steering wheel in the straight ahead driving position, and loosen the lock lever fully.

1. Attach the spring scale to the center point of the steering wheel.

1. Pull the spring scale, and read the force required to move the steering column during telescopic.

   Telescoping force:
   Standard: | 110 N (11.2 kgf, 24.7 lbf) max.

1. If the measurement is higher than the specified, replace the steering column as an assembly.

Check of Lock Lever Force

1. Move the lock lever (A) from the loosened position to the locked position three to five times, then release the lock lever. Adjust the steering column to the center tilt position and also to the full telescopic out position, and hold the steering wheel.

1. Using a push gauge, push the lock lever at 10 mm (0.39 in.) from its end, and measure the force required to move lock lever.

   Lock lever force:
   | 50−70 N (5.1−7.1 kgf, 11−16 lbf) min.

1. If the measurement is higher than the specified, replace the steering column as an assembly.