( TL19E20A14680200000KAAT00 )

Cylinder Head Valve, Spring, and Valve Seal Removal

Special Tools Required
Valve spring compressor
07757-0010000
Identify the valves and the valve springs as they are removed so that each item can be reinstalled in its original position.

1. Remove the cylinder head.

1. Using an appropriate-sized socket (A), and a plastic mallet (B), lightly tap the spring retainer to loosen the valve cotters.

1. Install valve the spring compressor. Compress the spring, and remove the valve cotters.

1. Remove the valve spring compressor, then remove the spring retainer, the valve spring, the valve seal, and the valve spring seat.