( TL19E00J54460647105FEAT01 )

Power Window Rear Motor Test - With All Power Windows AUTO UP/DOWN Function

With all power windows AUTO UP/AUTO DOWN function
Motor Test

1. Remove the rear power window switch.

1. Test the motor in each direction by connecting battery power and ground to the rear power window switch 14P connector (A) according to the table.

1. If the motor does not run or fails to run smoothly, go to Step 4 .

1. Remove the door panel.