( TL19E00J54460647101FEAT00 )

Power Window Driver's Motor Test

Pulser Test

1. Check for continuity between the driver's power window motor 6P connector No. 2 terminal and body ground. There should be continuity.
   - If there is continuity, go to Step 9 .
   - If there is no continuity, check for an open in the BLK wire or poor ground (G501).

1. Do the power window master switch input test No. 3, No. 20, and No. 22 terminals.