( TL19E00J18573560311KBAT00 )

Trunk Lid Latch Replacement

NOTE:

- Put on gloves to protect your hands.
- Take care not to scratch the trunk lid.
- When removing components, use the trim tools or equivalent.

1. If equipped, remove the trunk lid trim panel.

1. From the latch cover (A) opening, pry the cover to release the projections (B) of the trunk lid latch (C) with the appropriate trim tool while pulling the cover, and release the projections (D) of the cover from the latch, then remove the cover.

1. Disconnect the trunk lid latch connector (E), and remove the bolts, then remove the trunk lid latch.

1. Disconnect the trunk lid opener cable (A). Take care not to kink the cable.

1. Install the latch in the reverse order of removal, and note these items:
   - Make sure the connector is plugged in properly and the opener cable is connected properly.
   - Make sure the trunk lid opens properly and locks securely.
   - Fix the original position of the outer end of cable (A) on the trunk lid latch securely. And check the trunk lid latch operation: Make sure the trunk lid latch unlock when turning the trunk lid cylinder with a key. If necessary, adjust the position of the cable end.