( TL19E1PE10400013001KBAT00 )

ATF Replacement

1. Remove the ATF dipstick, and refill the transmission with the recommended fluid amount through the ATF dipstick guide tube opening (A) bring the fluid level between the upper mark and the lower mark on the ATF dipstick. Do not fill the fluid above the upper mark. Always use genuine Honda ATF-Z1 automatic transmission fluid (ATF). Using a non-Honda ATF can affect shift quality.

   Automatic Transmission Fluid Capacity:
   2.5 L (2.6 US qt, 2.2 Imp qt) at change
   6.5 L (6.9 US qt, 5.7 Imp qt) at overhaul